{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["BOM Report","Project Information"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM Report","index":0,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
[]
["Bill of Materials",null,"<Parameter Title not found>"]
["Source Data From:"]
["Project:"]
["Variant:"]
[]
["Creation Date:","2022-04-03"]
["Print Date:",{"$f":"TODAY()","v":"2022-04-03"}]
[]
[]
["Comment","Description","Designator","Value","Package","Quantity"]
["电容","贴片电容","C1, C2, C3, C4, C5, C6, C9, C15, C18, C19, C21, C24, C27, C31, C35, C36, C37, C42, C43, C44, C47, C50, C56","100nF 6.3V X7R 10%","0402",23]
["电容","贴片电容","C7, C8, C45, C46","100uF 6.3V X7R 20%","1206",4]
["电容","贴片电容","C10, C54","22nF 6.3V X7R 10%","0402",2]
["电容","贴片电容","C11, C13","6.8nF 6.3V X7R 10%","0402",2]
["电容","贴片电容","C12, C30","10nF 6.3V X7R 10%","0402",2]
["电容","钽电容","C14, C20","100uF 6.3V 20%","钽电容B型3528",2]
["电容","贴片电容","C16, C22, C32, C33, C34","33pF 6.3V NP0 2%","0402",5]
["电容","贴片电容","C17, C23","10pF 6.3V NP0 2%","0402",2]
["电容","钽电容","C25, C26","47uF 16V 20%","钽电容B型3528",2]
["电容","贴片电容","C28, C29","NC","0402",2]
["电容","贴片电容","C38, C39","7pF 6.3V NP0 2%","0402",2]
["电容","贴片电容","C40, C41","12pF 6.3V NP0 2%","0402",2]
["电容","贴片电容","C48","10uF 6.3V X7R 20%","0603",1]
["电容","贴片电容","C49","1uF 6.3V X7R 10%","0402",1]
["电容","固态电容","C51, C53","470uF 50V 20%","CAP-SMD_BD8.0-L8.4-W8.4-LS9.0-FD",2]
["电容","贴片电容","C52","100nF 50V X7R 10%","0603",1]
["电容","超级电容","C55","10F -10%~+20% 5.5V","32.5*36.5*16.5",1]
["WJ2EDGRC-5.08-2P","插拔式接线端子插座","CN1","WJ2EDGRC-5.08-2P","CONN-TH_2P-P5.08",1]
["SMAJ6.5CA","双向TVS","D1, D2, D3","SMAJ6.5CA","SMA",3]
["ESD","ESD 4.5V","D4","ESD56151W04-2/TR","SOD323",1]
["ESD","ESD芯片","D5","ESDA6V8AV6-6/TR","SOT-563",1]
["ABS10_C190798","","D6","","",1]
["SS54","肖特基二极管","D7, D8, D9","SS54","SMA",3]
["DC-005 5.5-2.0MM","","DC1","","",1]
["DMR-9S","DB9母座","DSUB1","D-DMR009PF-D002","DSUB-TH_DMR-9S",1]
["天线座","IPEX天线座","E1","IPEX 4代","IPEX",1]
["HR911105A_C12074","","J1","","",1]
["电感","功率电感","L1","3.3uH ±20% 5.5A 38mΩ","IND-SMD_L5.4-W5.2",1]
["LED0","Typical INFRARED GaAs LED","LED1, LED2, LED3, LED4, LED5","3mm直插led","",5]
["LED0","贴片LED","LED6","LED","0603",1]
["PTC","热恢复保险丝","PTC1, PTC2","30V 0.05A","1206",2]
["热恢复保险丝","热恢复保险丝","PTC3, PTC4","3A 16V","0603",2]
["S8050","NPN三极管","Q1","S8050","SOT-23",1]
["三极管","NPN贴片三极管","Q2, Q3, Q4, Q5, Q6","S8050","SOT-23",5]
["电阻","贴片电阻","R1, R2, R3, R6, R7, R19, R20, R26, R30, R36","4.7K 1/16W 1%","0402",10]
["电阻","贴片电阻","R4","120Ω 1/4W 1%","1206",1]
["电阻","贴片电阻","R5, R9, R10, R17, R18, R38, R39, R49, R51","1K 1/16W 1%","0402",9]
["电阻","贴片电阻","R8, R32, R33, R34","20Ω 1/16W 1%","0402",4]
["电阻","贴片电阻","R11, R12","51Ω 1/16W 1%","0402",2]
["电阻","贴片电阻","R13","10Ω 1/16W 1%","0402",1]
["电阻","贴片电阻","R14, R15","82Ω 1/16W 1%","0402",2]
["磁珠","贴片磁珠","R16","120R 100MHz 3A","0603",1]
["电阻","贴片电阻","R21, R22, R23, R25, R28, R31, R37","47K 1/16W 1%","0402",7]
["电阻","贴片电阻","R24","100K 1/16W 1%","0402",1]
["电阻","贴片电阻","R27, R29, R40, R41, R42, R43, R45","0Ω 1/16W 1%","0402",7]
["电阻","贴片电阻","R35","51K 1/16W 1%","0402",1]
["电阻","贴片电阻","R44, R46","10K 1/16W 1%","0402",2]
["电阻","贴片电阻","R47","12K 1/16W 1%","0402",1]
["电阻","贴片电阻","R48","2K 1/16W 1%","0402",1]
["电阻","贴片电阻","R50","2M 1/16W 1%","0402",1]
["电阻","贴片电阻","R52","1M 1/16W 1%","0402",1]
["轻触开关","卧贴轻触开关","SW1","SKRTLAE010","",1]
["MAX3485EESA","","U1","","",1]
["SP3232EEA-L/TR","RS232芯片","U2","SP3232EEA-L/TR","SSOP-16",1]
["电源芯片","LDO","U3, U9","ME6230C33M5G","SOT-23-5",2]
["RS0102YUTDS8","No Description Available","U4","RS0102YUTDS8","DFN1.4*1.0-8",1]
["EC200N-CN","EC200N-CN Module LCC80PIN LGA52PIN 32X29mm H2.4mm RO","U5","EC200N-CN","EC200N-CN",1]
["MIC29302WU","LDO Vin=26V Vout=1.25V~25V 3A","U6","MIC29302WU","",1]
["Sim卡座","Sim卡座","U7","Nano-Sim自弹卡座","",1]
["CH32V307VCT6","CH32V307VCT6","U8","CH32V307VCT6","LQFP-100",1]
["W25Q64JVSSIQ","Flash","U10","W25Q64JVSSIQ","SOIC-8",1]
["XL4005E1","","U11","","",1]
["TYPE-C16PIN","","USB1","","",1]
["晶振","贴片无源晶振","Y1","25MHz 4P 匹配电容12pF 10PPM","2016",1]
["晶振","贴片无源晶振","Y2","32.768KHz 2P 匹配电容7pF 10PPM","3215",1]
[{"$nulls":5},{"$f":"SUM(F12:F76)","v":154}]
["Approved",{"$nulls":5}," "]

{"sheet":"Project Information","index":1,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Project Full Path","D:\\git_workspace\\sanoh\\PLC_DTU\\PCB\\MAIN.PrjPcb"]
["Project Filename","MAIN.PrjPcb"]
["Variant Name","None"]
["Data-Source Filename","MAIN.PrjPcb"]
["Data-Source Full Path","D:\\git_workspace\\sanoh\\PLC_DTU\\PCB\\MAIN.PrjPcb"]
["Title","<Parameter Title not found>"]
["Total Quantity","167"]
["Report Time","14:01:28"]
["Report Date","2022-04-03"]
["Report Date & Tine","2022-04-03 14:01:28"]
["Output Name","Bill of Materials"]
["Output Type","BOM_PartType"]
["Output Generator Name","BOM"]
["Output Generator Description","Bill of Materials"]